** Drc report for MaA_psu.kicad_pcb **
** Created on 2026-04-02T19:46:02 **
** Report includes: Errors, Warnings, Exclusions **

** Found 514 DRC violations **
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(181.0500 mm, 104.5000 mm): Track [Net-(C10-Pad2)] on F.Cu, length 7.1771 mm
    @(183.6000 mm, 102.0000 mm): Pad 1 [<no net>] of OUT on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.5750 mm, 96.5760 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1760 mm
[solder_mask_bridge]: Front solder mask aperture bridges items with different nets
    Rule: board setup solder mask min width; error
    @(160.5180 mm, 97.5250 mm): Polygon of Q5 on F.Mask
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Power'; error
    @(150.6000 mm, 92.0000 mm): Via [-BATT] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Power'; error
    @(146.7000 mm, 100.0493 mm): Via [-BATT] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Power'; error
    @(157.4400 mm, 107.6000 mm): Via [-BATT] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Power'; error
    @(144.7500 mm, 102.5500 mm): Via [-BATT] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(194.6000 mm, 96.6000 mm): Via [Net-(J2-CC1)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(194.6000 mm, 95.4000 mm): Via [Net-(J2-CC2)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(152.8000 mm, 93.7916 mm): Via [Net-(U2-VSYS)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(171.4450 mm, 91.4037 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(171.0000 mm, 90.1000 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass '3A'; error
    @(141.4769 mm, 104.5231 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass '3A'; error
    @(143.5000 mm, 102.0000 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(132.2000 mm, 96.2600 mm): Via [/FUSB302 Interrupt] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(132.6933 mm, 95.9745 mm): Via [/SCL] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(148.2750 mm, 101.7922 mm): Via [/SCL] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(133.0823 mm, 95.5856 mm): Via [/SDA] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(148.2606 mm, 101.0806 mm): Via [/SDA] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(143.3418 mm, 93.0125 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(144.5652 mm, 100.4793 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(142.5481 mm, 99.4157 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(140.5000 mm, 90.9000 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(144.6132 mm, 94.7626 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(166.2000 mm, 118.3200 mm): Via [/CPU Throttle] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(144.9968 mm, 99.1968 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(143.1700 mm, 99.2614 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(154.3632 mm, 97.9916 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(142.3750 mm, 94.9850 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(146.4000 mm, 102.6000 mm): Via [Net-(U2-IADPT)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(146.4600 mm, 103.6000 mm): Via [Net-(U2-IBAT)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(149.9190 mm, 96.1192 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(146.5000 mm, 109.3000 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(145.6206 mm, 93.5787 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[via_diameter]: Via diameter (board setup constraints min diameter 0.5000 mm; actual 0.4000 mm)
    Rule: netclass 'Default'; error
    @(148.9553 mm, 92.7125 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(173.3350 mm, 97.2125 mm): Pad 7 [-BATT] of U4 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(131.4400 mm, 94.8300 mm): Pad 8 [-BATT] of U1 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(130.9400 mm, 94.8300 mm): Pad 9 [-BATT] of U1 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(139.8082 mm, 91.5666 mm): Pad 3 [-BATT] of Q4 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(153.6682 mm, 90.9166 mm): Pad 1 [-BATT] of Q1 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(143.0606 mm, 94.1394 mm): Pad 2 [-BATT] of C3 on F.Cu
[starved_thermal]: Thermal relief connection to zone incomplete (layer F.Cu; zone min spoke count 2; actual 1)
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(168.8000 mm, 91.9000 mm): Pad 2 [-BATT] of R11 on F.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(174.0000 mm, 94.0000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(172.7000 mm, 94.0000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(171.4000 mm, 94.0000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(174.0000 mm, 95.3000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(172.7000 mm, 95.3000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(171.4000 mm, 95.3000 mm): PTH pad 9 [-BATT] of U4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.0132 mm, 92.8666 mm): PTH pad 6 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.1082 mm, 92.8666 mm): PTH pad 7 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.4652 mm, 91.8916 mm): PTH pad 8 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.5602 mm, 91.8916 mm): PTH pad 9 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(136.6552 mm, 91.8916 mm): PTH pad 10 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.0132 mm, 90.9166 mm): PTH pad 11 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.1082 mm, 90.9166 mm): PTH pad 12 [/SW1] of Q4
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(159.0950 mm, 96.4000 mm): PTH pad 9_2 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(160.9050 mm, 96.4000 mm): PTH pad 9_5 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.0662 mm, 102.1666 mm): PTH pad 6 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.1612 mm, 102.1666 mm): PTH pad 7 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.5182 mm, 101.1916 mm): PTH pad 8 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.6132 mm, 101.1916 mm): PTH pad 9 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(136.7082 mm, 101.1916 mm): PTH pad 10 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(138.0662 mm, 100.2166 mm): PTH pad 11 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(137.1612 mm, 100.2166 mm): PTH pad 12 [Net-(U2-ACN)] of Q3
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 100.1666 mm): PTH pad 6 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 100.1666 mm): PTH pad 7 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.0112 mm, 101.1416 mm): PTH pad 8 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.9162 mm, 101.1416 mm): PTH pad 9 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.8212 mm, 101.1416 mm): PTH pad 10 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 102.1166 mm): PTH pad 11 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 102.1166 mm): PTH pad 12 [+BATT] of Q2
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 90.9166 mm): PTH pad 6 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 90.9166 mm): PTH pad 7 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.0112 mm, 91.8916 mm): PTH pad 8 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.9162 mm, 91.8916 mm): PTH pad 9 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.8212 mm, 91.8916 mm): PTH pad 10 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 92.8666 mm): PTH pad 11 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 92.8666 mm): PTH pad 12 [Net-(U2-SW2)] of Q1
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(150.6000 mm, 92.0000 mm): Via [-BATT] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(146.7000 mm, 100.0493 mm): Via [-BATT] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(157.4400 mm, 107.6000 mm): Via [-BATT] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.7500 mm, 102.5500 mm): Via [-BATT] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.1000 mm)
    Rule: netclass 'Power'; error
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(194.6000 mm, 96.6000 mm): Via [Net-(J2-CC1)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(194.6000 mm, 95.4000 mm): Via [Net-(J2-CC2)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(152.8000 mm, 93.7916 mm): Via [Net-(U2-VSYS)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(171.4450 mm, 91.4037 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(171.0000 mm, 90.1000 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass '3A'; error
    @(141.4769 mm, 104.5231 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass '3A'; error
    @(143.5000 mm, 102.0000 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(132.2000 mm, 96.2600 mm): Via [/FUSB302 Interrupt] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(132.6933 mm, 95.9745 mm): Via [/SCL] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(148.2750 mm, 101.7922 mm): Via [/SCL] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(133.0823 mm, 95.5856 mm): Via [/SDA] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(148.2606 mm, 101.0806 mm): Via [/SDA] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(143.3418 mm, 93.0125 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(144.5652 mm, 100.4793 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(142.5481 mm, 99.4157 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(140.5000 mm, 90.9000 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(144.6132 mm, 94.7626 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(166.2000 mm, 118.3200 mm): Via [/CPU Throttle] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(144.9968 mm, 99.1968 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(143.1700 mm, 99.2614 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(154.3632 mm, 97.9916 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(140.0481 mm, 99.8703 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(142.3750 mm, 94.9850 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(146.4000 mm, 102.6000 mm): Via [Net-(U2-IADPT)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(146.4600 mm, 103.6000 mm): Via [Net-(U2-IBAT)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(149.9190 mm, 96.1192 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(146.5000 mm, 109.3000 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(145.6206 mm, 93.5787 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[drill_out_of_range]: Hole size out of range (board setup constraints min hole 0.2500 mm; actual 0.2000 mm)
    Rule: netclass 'Default'; error
    @(148.9553 mm, 92.7125 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[courtyards_overlap]: Courtyards overlap
    Rule: board setup constraints courtyard; error
    @(161.0000 mm, 104.8000 mm): Footprint R17
    @(155.2182 mm, 101.1416 mm): Footprint Q2
[shorting_items]: Items shorting two nets (nets Net-(U2-SRP) and )
    Local override; error
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2012 mm)
    Rule: netclass 'Power'; error
    @(137.6132 mm, 91.8916 mm): Pad 5 [/SW1] of Q4 on F.Cu
    @(134.2000 mm, 92.3148 mm): Track [+3.3V] on F.Cu, length 5.9606 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2211 mm)
    Rule: netclass 'Power'; error
    @(145.7025 mm, 94.6908 mm): Pad 27 [-BATT] of U2 on F.Cu
    @(144.1643 mm, 93.7128 mm): Track [Net-(U2-REGN)] on F.Cu, length 1.7753 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1319 mm)
    Rule: netclass 'Power'; error
    @(141.2981 mm, 100.7587 mm): Track [/SW1] on F.Cu, length 1.3606 mm
    @(142.5000 mm, 99.4150 mm): Pad 1 [Net-(U2-REGN)] of R3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2389 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
    @(131.8800 mm, 97.0000 mm): Track [+3.3V] on F.Cu, length 0.3394 mm
[clearance]: Clearance violation (netclass '3A' clearance 0.2000 mm; actual 0.1994 mm)
    Rule: netclass '3A'; error
    @(130.9000 mm, 97.3000 mm): Polygon [Net-(TVS1-A1)] on F.Cu
    @(131.4400 mm, 97.1900 mm): Track [+3.3V] on F.Cu, length 0.2500 mm
[shorting_items]: Items shorting two nets (nets Net-(C10-Pad2) and )
    Local override; error
    @(181.0500 mm, 104.5000 mm): Track [Net-(C10-Pad2)] on F.Cu, length 7.1771 mm
    @(183.6000 mm, 102.0000 mm): Pad 1 [<no net>] of OUT on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2650 mm)
    Rule: netclass 'Power'; error
    @(130.8800 mm, 93.9700 mm): Rectangle [-BATT] on F.Cu
    @(130.1900 mm, 94.8300 mm): Track [Net-(J1-CC1)] on F.Cu, length 0.2500 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2718 mm)
    Rule: netclass 'Power'; error
    @(161.4000 mm, 101.5000 mm): Via [-BATT] on F.Cu - B.Cu
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(141.2981 mm, 100.7587 mm): Track [/SW1] on F.Cu, length 1.3606 mm
    @(140.0481 mm, 99.8703 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2250 mm)
    Rule: netclass 'Power'; error
    @(145.0148 mm, 99.1968 mm): Track [Net-(U2-ILIM_HIZ)] on F.Cu, length 0.9725 mm
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(140.2216 mm, 101.5000 mm): Track [/SW1] on F.Cu, length 0.3504 mm
    @(137.6662 mm, 101.1916 mm): Pad 5 [Net-(U2-ACN)] of Q3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(156.0000 mm, 108.8000 mm): Rectangle [+BATT] on F.Cu
    @(158.0000 mm, 108.2500 mm): Via [/Fuel Gauge Alert] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(149.1201 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6332 mm
    @(148.3895 mm, 95.2565 mm): Track [Net-(U2-SRP)] on F.Cu, length 0.1061 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2883 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
    @(132.3800 mm, 97.5600 mm): Track [+3.3V] on F.Cu, length 0.7071 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1493 mm)
    Rule: netclass 'Power'; error
    @(142.5000 mm, 100.4350 mm): Pad 2 [Net-(U2-ILIM_HIZ)] of R3 on F.Cu
    @(140.5569 mm, 101.5000 mm): Track [/SW1] on F.Cu, length 1.0483 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2661 mm)
    Rule: netclass 'Power'; error
    @(144.9900 mm, 99.2000 mm): Pad 2 [Net-(U2-ILIM_HIZ)] of R4 on B.Cu
    @(145.4197 mm, 98.2263 mm): Track [-BATT] on B.Cu, length 0.3833 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2880 mm)
    Rule: netclass 'Power'; error
    @(149.7916 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6715 mm
    @(148.3895 mm, 95.2565 mm): Pad 20 [Net-(U2-SRP)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2600 mm)
    Rule: netclass 'Power'; error
    @(144.9900 mm, 99.2000 mm): Pad 2 [Net-(U2-ILIM_HIZ)] of R4 on B.Cu
    @(145.4197 mm, 98.6097 mm): Track [-BATT] on B.Cu, length 0.8349 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2556 mm)
    Rule: netclass 'Power'; error
    @(149.7916 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6715 mm
    @(149.9190 mm, 95.7190 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.3137 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2389 mm)
    Rule: netclass 'Power'; error
    @(137.1612 mm, 102.1666 mm): PTH pad 7 [Net-(U2-ACN)] of Q3
    @(137.2672 mm, 101.6166 mm): Track [/FUSB302 Interrupt] on B.Cu, length 0.5289 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2863 mm)
    Rule: netclass 'Power'; error
    @(137.1612 mm, 102.1666 mm): PTH pad 7 [Net-(U2-ACN)] of Q3
    @(137.6412 mm, 102.3426 mm): Track [/FUSB302 Interrupt] on B.Cu, length 18.8124 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2556 mm)
    Rule: netclass 'Power'; error
    @(149.7916 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6715 mm
    @(149.3905 mm, 95.4972 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.0984 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(136.7082 mm, 101.1916 mm): PTH pad 10 [Net-(U2-ACN)] of Q3
    @(133.0000 mm, 98.0845 mm): Track [/FUSB302 Interrupt] on B.Cu, length 4.9952 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2036 mm)
    Rule: netclass 'Power'; error
    @(149.9190 mm, 95.7190 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.3137 mm
    @(150.6358 mm, 95.9358 mm): Track [+BATT] on F.Cu, length 1.1939 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2405 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
    @(131.8800 mm, 97.0600 mm): Track [+3.3V] on F.Cu, length 0.0600 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2036 mm)
    Rule: netclass 'Power'; error
    @(150.6358 mm, 95.9358 mm): Track [+BATT] on F.Cu, length 1.1939 mm
    @(149.9190 mm, 96.1192 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.4002 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2405 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
    @(131.6900 mm, 97.1900 mm): Track [+3.3V] on F.Cu, length 0.2687 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2250 mm)
    Rule: netclass 'Power'; error
    @(149.1201 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6332 mm
    @(148.3895 mm, 95.2565 mm): Pad 20 [Net-(U2-SRP)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2969 mm)
    Rule: netclass 'Power'; error
    @(149.1201 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6332 mm
    @(149.3025 mm, 95.5412 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.3974 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(155.5000 mm, 116.7700 mm): PTH pad 2 [-BATT] of J3
    @(150.9435 mm, 115.6450 mm): Track [/FUSB302 Interrupt] on B.Cu, length 11.4215 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2550 mm)
    Rule: netclass 'Power'; error
    @(137.1612 mm, 102.1666 mm): PTH pad 7 [Net-(U2-ACN)] of Q3
    @(137.6412 mm, 101.9905 mm): Track [/FUSB302 Interrupt] on B.Cu, length 0.3521 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(149.1201 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6332 mm
    @(149.0215 mm, 95.8222 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.0663 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(136.7082 mm, 101.1916 mm): PTH pad 10 [Net-(U2-ACN)] of Q3
    @(136.5321 mm, 101.6166 mm): Track [/FUSB302 Interrupt] on B.Cu, length 0.7351 mm
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.1428 mm)
    Rule: netclass 'Default'; error
    @(144.7888 mm, 95.5393 mm): Track [Net-(U2-BTST1)] on F.Cu, length 0.8495 mm
    @(144.6000 mm, 95.8000 mm): Segment [Net-(Q3-G)] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2556 mm)
    Rule: netclass 'Power'; error
    @(149.7916 mm, 95.0916 mm): Track [+BATT] on F.Cu, length 0.6715 mm
    @(149.6972 mm, 95.4972 mm): Track [Net-(J3b1-Pin_2)] on F.Cu, length 0.3067 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2250 mm)
    Rule: netclass 'Power'; error
    @(146.9632 mm, 93.8302 mm): Track [Net-(Q2-G)] on F.Cu, length 0.4172 mm
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.1428 mm)
    Rule: netclass 'Default'; error
    @(144.6000 mm, 95.8000 mm): Segment [Net-(Q3-G)] on F.Cu
    @(144.8540 mm, 95.5393 mm): Track [Net-(U2-BTST1)] on F.Cu, length 0.0651 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2211 mm)
    Rule: netclass 'Power'; error
    @(145.7025 mm, 94.6908 mm): Pad 27 [-BATT] of U2 on F.Cu
    @(145.4197 mm, 94.9681 mm): Track [Net-(U2-REGN)] on F.Cu, length 0.0056 mm
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(130.4400 mm, 97.1900 mm): Pad 1 [Net-(J1-CC2)] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2243 mm)
    Rule: netclass 'Power'; error
    @(144.2883 mm, 97.0950 mm): Pad 1 [Net-(U2-ACN)] of U2 on F.Cu
    @(144.2883 mm, 96.1050 mm): Pad 32 [/SW1] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 97.1900 mm): Pad 2 [Net-(TVS1-A1)] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.2883 mm, 97.0950 mm): Pad 1 [Net-(U2-ACN)] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(153.6682 mm, 101.4666 mm): Pad 3 [Net-(U2-SW2)] of Q2 on F.Cu
    @(153.6682 mm, 102.1166 mm): Pad 4 [Net-(Q2-G)] of Q2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(131.4400 mm, 97.1900 mm): Pad 3 [+3.3V] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(160.9050 mm, 96.4000 mm): PTH pad 9_5 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(139.8612 mm, 100.8666 mm): Pad 3 [/SW1] of Q3 on F.Cu
    @(139.8612 mm, 100.2166 mm): Pad 4 [Net-(Q3-G)] of Q3 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.9402 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2794 mm)
    Rule: netclass 'Power'; error
    @(144.5711 mm, 97.3778 mm): Pad 2 [Net-(U2-ACN)] of U2 on F.Cu
    @(145.3263 mm, 96.6000 mm): PTH pad P$1 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.5711 mm, 97.3778 mm): Pad 2 [Net-(U2-ACN)] of U2 on F.Cu
    @(144.8540 mm, 97.6607 mm): Pad 3 [Net-(TVS1-A1)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(139.8082 mm, 91.5666 mm): Pad 3 [-BATT] of Q4 on F.Cu
    @(139.8082 mm, 90.9166 mm): Pad 4 [Net-(Q4-G)] of Q4 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.5711 mm, 97.3778 mm): Pad 2 [Net-(U2-ACN)] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0513 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(159.0950 mm, 96.4000 mm): PTH pad 9_2 [<no net>] of Q5
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(159.9480 mm, 96.4000 mm): Pad 9 [Net-(U2-SRP)] of Q5 on F.Cu
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1750 mm)
    Rule: board setup constraints hole; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1750 mm)
    Rule: board setup constraints hole; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(132.1200 mm, 96.7600 mm): Pad 4 [+3.3V] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(132.1200 mm, 96.2600 mm): Pad 5 [/FUSB302 Interrupt] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1623 mm)
    Rule: board setup constraints hole; error
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1631 mm)
    Rule: board setup constraints hole; error
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(132.1200 mm, 95.7600 mm): Pad 6 [/SCL] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1623 mm)
    Rule: board setup constraints hole; error
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2871 mm)
    Rule: netclass 'Power'; error
    @(132.1200 mm, 95.2600 mm): Pad 7 [/SDA] of U1 on F.Cu
    @(131.4400 mm, 94.8300 mm): Pad 8 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(174.6050 mm, 92.0875 mm): Pad 1 [Net-(U4-BOOT)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(132.1200 mm, 95.2600 mm): Pad 7 [/SDA] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[hole_clearance]: Hole clearance violation (board setup constraints hole clearance 0.2500 mm; actual 0.1631 mm)
    Rule: board setup constraints hole; error
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(173.3350 mm, 92.0875 mm): Pad 2 [Net-(U2-VSYS)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2200 mm)
    Rule: netclass 'Power'; error
    @(130.9400 mm, 94.8300 mm): Pad 9 [-BATT] of U1 on F.Cu
    @(130.4400 mm, 94.8300 mm): Pad 10 [Net-(J1-CC1)] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(172.0650 mm, 92.0875 mm): Pad 3 [Net-(U4-EN)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(170.7950 mm, 92.0875 mm): Pad 4 [Net-(U4-RT/CLK)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(130.4400 mm, 94.8300 mm): Pad 10 [Net-(J1-CC1)] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(170.7950 mm, 97.2125 mm): Pad 5 [Net-(U4-FB)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(129.7600 mm, 95.2600 mm): Pad 11 [Net-(J1-CC1)] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(129.7600 mm, 95.7600 mm): Pad 12 [+3.3V] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(172.0650 mm, 97.2125 mm): Pad 6 [Net-(U4-COMP)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(129.7600 mm, 96.2600 mm): Pad 13 [+3.3V] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2350 mm)
    Rule: netclass 'Power'; error
    @(129.7600 mm, 96.7600 mm): Pad 14 [Net-(J1-CC2)] of U1 on F.Cu
    @(130.9400 mm, 96.0100 mm): Pad 15 [-BATT] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(174.6050 mm, 97.2125 mm): Pad 8 [Net-(D1-K)] of U4 on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(162.0938 mm, 108.8000 mm): Pad 1 [unconnected-(U3-N.C.-Pad1)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(162.0938 mm, 108.4000 mm): Pad 2 [unconnected-(U3-AIN-Pad2)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(162.0938 mm, 108.0000 mm): Pad 3 [/SCL] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(162.0938 mm, 107.6000 mm): Pad 4 [/SDA] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(162.0938 mm, 107.2000 mm): Pad 5 [Net-(U3-CSN)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 107.2000 mm): Pad 6 [Net-(U3-CSP)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 107.6000 mm): Pad 7 [Net-(U3-REG)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 108.0000 mm): Pad 8 [/Fuel Gauge Alert] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 108.4000 mm): Pad 9 [unconnected-(U3-THRM-Pad9)] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1968 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 108.4000 mm): Pad 9 [unconnected-(U3-THRM-Pad9)] of U3 on F.Cu
    @(159.7062 mm, 108.8000 mm): Pad 10 [+BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1905 mm)
    Rule: netclass 'Power'; error
    @(159.7062 mm, 108.8000 mm): Pad 10 [+BATT] of U3 on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(148.9552 mm, 95.8222 mm): Pad 18 [Net-(J3b1-Pin_2)] of U2 on F.Cu
    @(148.6723 mm, 95.5393 mm): Pad 19 [+BATT] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(148.6723 mm, 95.5393 mm): Pad 19 [+BATT] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(148.6723 mm, 95.5393 mm): Pad 19 [+BATT] of U2 on F.Cu
    @(148.3895 mm, 95.2565 mm): Pad 20 [Net-(U2-SRP)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(147.8238 mm, 94.6908 mm): Pad 22 [Net-(U2-VSYS)] of U2 on F.Cu
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2794 mm)
    Rule: netclass 'Power'; error
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
    @(146.7632 mm, 95.1632 mm): PTH pad P$3 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
    @(147.2581 mm, 94.1251 mm): Pad 24 [Net-(Q2-G)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(145.9853 mm, 94.4080 mm): Pad 26 [Net-(Q1-G)] of U2 on F.Cu
    @(145.7025 mm, 94.6908 mm): Pad 27 [-BATT] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(145.7025 mm, 94.6908 mm): Pad 27 [-BATT] of U2 on F.Cu
    @(145.4197 mm, 94.9737 mm): Pad 28 [Net-(U2-REGN)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(145.7025 mm, 94.6908 mm): Pad 27 [-BATT] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.5711 mm, 95.8222 mm): Pad 31 [Net-(Q3-G)] of U2 on F.Cu
    @(144.2883 mm, 96.1050 mm): Pad 32 [/SW1] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(144.2883 mm, 96.1050 mm): Pad 32 [/SW1] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(146.7632 mm, 98.0368 mm): PTH pad P$4 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(146.0447 mm, 95.8816 mm): PTH pad P$2 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(146.7632 mm, 95.1632 mm): PTH pad P$3 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(145.3263 mm, 96.6000 mm): PTH pad P$1 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(146.7632 mm, 96.6000 mm): PTH pad P$7 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(146.0447 mm, 97.3184 mm): PTH pad P$9 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(147.4816 mm, 97.3184 mm): PTH pad P$6 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(147.4816 mm, 95.8816 mm): PTH pad P$8 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND [<no net>] of U2 on F.Cu
    @(148.2000 mm, 96.6000 mm): PTH pad P$5 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(146.0447 mm, 95.8816 mm): PTH pad P$2 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(146.7632 mm, 95.1632 mm): PTH pad P$3 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(148.2000 mm, 96.6000 mm): PTH pad P$5 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(147.4816 mm, 95.8816 mm): PTH pad P$8 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(146.7632 mm, 98.0368 mm): PTH pad P$4 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(147.4816 mm, 97.3184 mm): PTH pad P$6 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(146.7632 mm, 96.6000 mm): PTH pad P$7 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(146.0447 mm, 97.3184 mm): PTH pad P$9 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.0000 mm)
    Rule: netclass 'Default'; error
    @(146.7632 mm, 96.6000 mm): Pad GND1 [<no net>] of U2 on B.Cu
    @(145.3263 mm, 96.6000 mm): PTH pad P$1 [<no net>] of U2
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2500 mm)
    Rule: netclass 'Power'; error
    @(153.6682 mm, 92.2166 mm): Pad 3 [-BATT] of Q1 on F.Cu
    @(153.6682 mm, 92.8666 mm): Pad 4 [Net-(Q1-G)] of Q1 on F.Cu
[clearance]: Clearance violation (netclass '3A' clearance 0.2000 mm; actual 0.1433 mm)
    Rule: netclass '3A'; error
    @(130.9000 mm, 97.3000 mm): Polygon [Net-(TVS1-A1)] on F.Cu
    @(130.4400 mm, 97.1900 mm): Pad 1 [Net-(J1-CC2)] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(145.9853 mm, 94.4080 mm): Pad 26 [Net-(Q1-G)] of U2 on F.Cu
    @(145.6997 mm, 94.6880 mm): Segment [-BATT] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2361 mm)
    Rule: netclass 'Power'; error
    @(144.6000 mm, 95.8000 mm): Segment [Net-(Q3-G)] on F.Cu
    @(144.2883 mm, 96.1050 mm): Pad 32 [/SW1] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1966 mm)
    Rule: netclass 'Power'; error
    @(145.4197 mm, 94.9737 mm): Pad 28 [Net-(U2-REGN)] of U2 on F.Cu
    @(145.6997 mm, 94.6880 mm): Segment [-BATT] on F.Cu
[clearance]: Clearance violation (netclass '3A' clearance 0.2000 mm; actual 0.1247 mm)
    Rule: netclass '3A'; error
    @(131.4400 mm, 97.1900 mm): Pad 3 [+3.3V] of U1 on F.Cu
    @(130.9000 mm, 97.3000 mm): Polygon [Net-(TVS1-A1)] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2007 mm)
    Rule: netclass 'Power'; error
    @(147.5500 mm, 94.4000 mm): Segment [Net-(U2-SW2)] on F.Cu
    @(147.2581 mm, 94.1251 mm): Pad 24 [Net-(Q2-G)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1720 mm)
    Rule: netclass 'Power'; error
    @(156.0000 mm, 108.8000 mm): Rectangle [+BATT] on F.Cu
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1897 mm)
    Rule: netclass 'Power'; error
    @(144.4000 mm, 98.1000 mm): Segment [Net-(TVS1-A1)] on F.Cu
    @(144.5711 mm, 97.3778 mm): Pad 2 [Net-(U2-ACN)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1834 mm)
    Rule: netclass 'Power'; error
    @(139.8612 mm, 100.2166 mm): Pad 4 [Net-(Q3-G)] of Q3 on F.Cu
    @(139.6000 mm, 100.7000 mm): Rectangle [/SW1] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2596 mm)
    Rule: netclass 'Power'; error
    @(148.0000 mm, 94.6000 mm): Segment [Net-(U2-VSYS)] on F.Cu
    @(147.5500 mm, 94.4000 mm): Segment [Net-(U2-SW2)] on F.Cu
[clearance]: Clearance violation (netclass '3A' clearance 0.2000 mm; actual 0.1927 mm)
    Rule: netclass '3A'; error
    @(144.8540 mm, 97.6607 mm): Pad 3 [Net-(TVS1-A1)] of U2 on F.Cu
    @(144.7200 mm, 98.3500 mm): Segment [/Charge Status] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2000 mm)
    Rule: netclass 'Power'; error
    @(130.8800 mm, 93.9700 mm): Rectangle [-BATT] on F.Cu
    @(130.4400 mm, 94.8300 mm): Pad 10 [Net-(J1-CC1)] of U1 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1984 mm)
    Rule: netclass 'Power'; error
    @(156.0000 mm, 108.8000 mm): Rectangle [+BATT] on F.Cu
    @(159.7062 mm, 108.4000 mm): Pad 9 [unconnected-(U3-THRM-Pad9)] of U3 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1464 mm)
    Rule: netclass 'Power'; error
    @(174.6050 mm, 97.2125 mm): Pad 8 [Net-(D1-K)] of U4 on F.Cu
    @(173.5250 mm, 96.6250 mm): Polygon [-BATT] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1750 mm)
    Rule: netclass 'Power'; error
    @(174.4000 mm, 96.4000 mm): Rectangle [Net-(D1-K)] on F.Cu
    @(172.7000 mm, 94.6500 mm): Pad 9 [-BATT] of U4 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1993 mm)
    Rule: netclass 'Power'; error
    @(147.5500 mm, 94.4000 mm): Segment [Net-(U2-SW2)] on F.Cu
    @(147.8238 mm, 94.6908 mm): Pad 22 [Net-(U2-VSYS)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2604 mm)
    Rule: netclass 'Power'; error
    @(148.0000 mm, 94.6000 mm): Segment [Net-(U2-VSYS)] on F.Cu
    @(147.5410 mm, 94.4080 mm): Pad 23 [Net-(U2-SW2)] of U2 on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.2375 mm)
    Rule: netclass 'Power'; error
    @(173.0000 mm, 98.8000 mm): Pad 1 [Net-(U4-COMP)] of C14 on F.Cu
    @(173.5250 mm, 96.6250 mm): Polygon [-BATT] on F.Cu
[clearance]: Clearance violation (netclass 'Power' clearance 0.3000 mm; actual 0.1272 mm)
    Rule: netclass 'Power'; error
    @(174.4000 mm, 96.4000 mm): Rectangle [Net-(D1-K)] on F.Cu
    @(173.5250 mm, 96.6250 mm): Polygon [-BATT] on F.Cu
[clearance]: Clearance violation (netclass 'Default' clearance 0.1500 mm; actual 0.1396 mm)
    Rule: netclass 'Default'; error
    @(148.0000 mm, 94.6000 mm): Segment [Net-(U2-VSYS)] on F.Cu
    @(148.1067 mm, 94.9737 mm): Pad 21 [Net-(U2-BATDRV_N)] of U2 on F.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.9050 mm, 96.4000 mm): PTH pad 9_5 [<no net>] of Q5
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[shorting_items]: Items shorting two nets (nets Net-(U2-SRP) and )
    Local override; error
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[shorting_items]: Items shorting two nets (nets  and Net-(U2-SRP))
    Local override; error
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
[shorting_items]: Items shorting two nets (nets Net-(U2-SRP) and )
    Local override; error
    @(158.8000 mm, 95.2000 mm): Polygon [Net-(U2-SRP)] on B.Cu
    @(159.0950 mm, 96.4000 mm): PTH pad 9_2 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(150.6000 mm, 92.0000 mm): Via [-BATT] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(146.7000 mm, 100.0493 mm): Via [-BATT] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(157.4400 mm, 107.6000 mm): Via [-BATT] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(144.7500 mm, 102.5500 mm): Via [-BATT] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(194.6000 mm, 96.6000 mm): Via [Net-(J2-CC1)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(194.6000 mm, 95.4000 mm): Via [Net-(J2-CC2)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(152.8000 mm, 93.7916 mm): Via [Net-(U2-VSYS)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(171.4450 mm, 91.4037 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(171.0000 mm, 90.1000 mm): Via [Net-(U4-EN)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(141.4769 mm, 104.5231 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(143.5000 mm, 102.0000 mm): Via [Net-(TVS1-A1)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1500 mm)
    Rule: board setup constraints; error
    @(132.3800 mm, 97.5600 mm): Via [+3.3V] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1500 mm)
    Rule: board setup constraints; error
    @(128.8800 mm, 96.0000 mm): Via [+3.3V] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(132.2000 mm, 96.2600 mm): Via [/FUSB302 Interrupt] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(132.6933 mm, 95.9745 mm): Via [/SCL] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(148.2750 mm, 101.7922 mm): Via [/SCL] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(133.0823 mm, 95.5856 mm): Via [/SDA] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(148.2606 mm, 101.0806 mm): Via [/SDA] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(158.0000 mm, 108.2500 mm): Via [/Fuel Gauge Alert] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(143.3418 mm, 93.0125 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(144.5652 mm, 100.4793 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(142.5481 mm, 99.4157 mm): Via [Net-(U2-REGN)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(140.5000 mm, 90.9000 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(144.6132 mm, 94.7626 mm): Via [Net-(Q4-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(166.2000 mm, 118.3200 mm): Via [/CPU Throttle] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(171.2000 mm, 118.4000 mm): Via [/Charge Status] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(144.9968 mm, 99.1968 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(143.1700 mm, 99.2614 mm): Via [Net-(U2-ILIM_HIZ)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(154.3632 mm, 97.9916 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1500 mm)
    Rule: board setup constraints; error
    @(140.0481 mm, 99.8703 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(142.3750 mm, 94.9850 mm): Via [Net-(Q3-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1500 mm)
    Rule: board setup constraints; error
    @(152.5241 mm, 102.2166 mm): Via [Net-(Q2-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1500 mm)
    Rule: board setup constraints; error
    @(146.9632 mm, 93.3916 mm): Via [Net-(Q2-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(146.4000 mm, 102.6000 mm): Via [Net-(U2-IADPT)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(146.4600 mm, 103.6000 mm): Via [Net-(U2-IBAT)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(149.9190 mm, 96.1192 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(146.5000 mm, 109.3000 mm): Via [Net-(J3b1-Pin_2)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(145.6206 mm, 93.5787 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1000 mm)
    Rule: board setup constraints; error
    @(148.9553 mm, 92.7125 mm): Via [Net-(Q1-G)] on F.Cu - B.Cu
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.0132 mm, 92.8666 mm): PTH pad 6 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.1082 mm, 92.8666 mm): PTH pad 7 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.4652 mm, 91.8916 mm): PTH pad 8 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.5602 mm, 91.8916 mm): PTH pad 9 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(136.6552 mm, 91.8916 mm): PTH pad 10 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.0132 mm, 90.9166 mm): PTH pad 11 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.1082 mm, 90.9166 mm): PTH pad 12 [/SW1] of Q4
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(160.0000 mm, 96.4000 mm): PTH pad 9_1 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(159.0950 mm, 96.4000 mm): PTH pad 9_2 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(160.9050 mm, 96.4000 mm): PTH pad 9_5 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0750 mm)
    Rule: board setup constraints; error
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.0662 mm, 102.1666 mm): PTH pad 6 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.1612 mm, 102.1666 mm): PTH pad 7 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.5182 mm, 101.1916 mm): PTH pad 8 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.6132 mm, 101.1916 mm): PTH pad 9 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(136.7082 mm, 101.1916 mm): PTH pad 10 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(138.0662 mm, 100.2166 mm): PTH pad 11 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(137.1612 mm, 100.2166 mm): PTH pad 12 [Net-(U2-ACN)] of Q3
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 100.1666 mm): PTH pad 6 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 100.1666 mm): PTH pad 7 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.0112 mm, 101.1416 mm): PTH pad 8 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.9162 mm, 101.1416 mm): PTH pad 9 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.8212 mm, 101.1416 mm): PTH pad 10 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 102.1166 mm): PTH pad 11 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 102.1166 mm): PTH pad 12 [+BATT] of Q2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(145.3263 mm, 96.6000 mm): PTH pad P$1 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(146.0447 mm, 95.8816 mm): PTH pad P$2 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(146.7632 mm, 95.1632 mm): PTH pad P$3 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(146.7632 mm, 98.0368 mm): PTH pad P$4 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(148.2000 mm, 96.6000 mm): PTH pad P$5 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(147.4816 mm, 97.3184 mm): PTH pad P$6 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(146.7632 mm, 96.6000 mm): PTH pad P$7 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(147.4816 mm, 95.8816 mm): PTH pad P$8 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.1798 mm)
    Rule: board setup constraints; error
    @(146.0447 mm, 97.3184 mm): PTH pad P$9 [<no net>] of U2
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 90.9166 mm): PTH pad 6 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 90.9166 mm): PTH pad 7 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.0112 mm, 91.8916 mm): PTH pad 8 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.9162 mm, 91.8916 mm): PTH pad 9 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.8212 mm, 91.8916 mm): PTH pad 10 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(155.4632 mm, 92.8666 mm): PTH pad 11 [Net-(U2-SW2)] of Q1
[annular_width]: Annular width (board setup constraints min annular width 0.2500 mm; actual 0.0500 mm)
    Rule: board setup constraints; error
    @(156.3682 mm, 92.8666 mm): PTH pad 12 [Net-(U2-SW2)] of Q1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(144.7300 mm, 100.3700 mm): Reference field of C16
    @(144.5732 mm, 100.1979 mm): Segment of R18 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(143.6700 mm, 99.9250 mm): Reference field of R3
    @(144.7300 mm, 100.3700 mm): Reference field of C16
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(143.0632 mm, 101.4916 mm): Segment of L1 on F.Silkscreen
    @(144.7300 mm, 100.3700 mm): Reference field of C16
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(129.6100 mm, 97.0900 mm): Segment of U1 on F.Silkscreen
    @(129.2000 mm, 97.8000 mm): Reference field of TVS1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(129.6100 mm, 97.3400 mm): Segment of U1 on F.Silkscreen
    @(129.2000 mm, 97.8000 mm): Reference field of TVS1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(130.4400 mm, 97.7400 mm): Circle of U1 on F.Silkscreen
    @(129.2000 mm, 97.8000 mm): Reference field of TVS1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(146.7632 mm, 100.7416 mm): Reference field of L1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.2500 mm, 100.4778 mm): Segment of C16 on F.Silkscreen
    @(146.7632 mm, 100.7416 mm): Reference field of L1
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(143.0632 mm, 101.4916 mm): Segment of L1 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(145.5300 mm, 100.4778 mm): Segment of C16 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.2500 mm, 100.4778 mm): Segment of C16 on F.Silkscreen
    @(146.1232 mm, 100.3516 mm): Reference field of R18
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(146.7632 mm, 99.5345 mm): Segment of U2 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(144.6645 mm, 93.8791 mm): Reference field of U2
    @(144.2202 mm, 94.6202 mm): Reference field of C3
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(127.2000 mm, 92.5800 mm): Reference field of C29
    @(127.4613 mm, 92.1650 mm): Segment of C15 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(177.1600 mm, 94.6000 mm): Reference field of C9
    @(176.1000 mm, 94.6500 mm): Reference field of U4
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(176.3600 mm, 94.4922 mm): Segment of C9 on F.Silkscreen
    @(176.1000 mm, 94.6500 mm): Reference field of U4
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(187.6000 mm, 93.9000 mm): Reference field of C12
    @(188.3113 mm, 93.4400 mm): Segment of C11 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(181.0000 mm, 99.2500 mm): Reference field of L2
    @(174.3500 mm, 98.7900 mm): Segment of D1 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(181.0000 mm, 99.2500 mm): Reference field of L2
    @(180.8500 mm, 98.7900 mm): Segment of D1 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(187.6000 mm, 97.1000 mm): Reference field of C11
    @(188.3113 mm, 96.6400 mm): Segment of C10 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(161.4965 mm, 106.8697 mm): Segment of U3 on F.Silkscreen
    @(161.0000 mm, 107.4300 mm): Reference field of R17
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(160.9000 mm, 108.0000 mm): Reference field of U3
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(169.6300 mm, 99.7000 mm): Reference field of R5
    @(169.1464 mm, 99.5800 mm): Segment of R6 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(174.3500 mm, 98.7900 mm): Segment of D1 on F.Silkscreen
    @(174.1600 mm, 99.2800 mm): Reference field of C14
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(172.5200 mm, 99.7400 mm): Reference field of C13
    @(173.0700 mm, 99.3000 mm): Reference field of R7
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(174.1600 mm, 99.2800 mm): Reference field of C14
    @(173.0700 mm, 99.3000 mm): Reference field of R7
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(172.6400 mm, 99.1722 mm): Segment of C14 on F.Silkscreen
    @(173.0700 mm, 99.3000 mm): Reference field of R7
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(174.1600 mm, 99.2800 mm): Reference field of C14
    @(172.5200 mm, 99.7400 mm): Reference field of C13
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(172.5200 mm, 99.7400 mm): Reference field of C13
    @(173.3600 mm, 99.1722 mm): Segment of C14 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(172.6400 mm, 99.1722 mm): Segment of C14 on F.Silkscreen
    @(172.5200 mm, 99.7400 mm): Reference field of C13
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(172.2800 mm, 99.1464 mm): Segment of R7 on F.Silkscreen
    @(172.5200 mm, 99.7400 mm): Reference field of C13
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.5200 mm, 99.1464 mm): Segment of R7 on F.Silkscreen
    @(172.5200 mm, 99.7400 mm): Reference field of C13
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.1800 mm, 99.8536 mm): Segment of R5 on F.Silkscreen
    @(172.5200 mm, 99.7400 mm): Reference field of C13
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(160.5600 mm, 92.7113 mm): Segment of C7 on F.Silkscreen
    @(159.9380 mm, 93.2250 mm): Reference field of Q5
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(156.2400 mm, 86.3200 mm): Reference field of C25
    @(155.2400 mm, 86.3200 mm): Reference field of C21
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(156.2400 mm, 86.3200 mm): Reference field of C25
    @(157.2400 mm, 86.3200 mm): Reference field of C24
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(156.7600 mm, 86.4278 mm): Segment of C21 on F.Silkscreen
    @(157.2400 mm, 86.3200 mm): Reference field of C24
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(155.5000 mm, 112.9000 mm): Segment of J3 on F.Silkscreen
    @(154.2000 mm, 112.7800 mm): Reference field of C30
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(154.2000 mm, 110.7800 mm): Reference field of C28
    @(155.5000 mm, 111.4600 mm): Reference field of J3
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(154.4613 mm, 110.3650 mm): Segment of C30 on F.Silkscreen
    @(154.2000 mm, 110.7800 mm): Reference field of C28
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(156.2400 mm, 86.3200 mm): Reference field of C25
    @(156.7600 mm, 86.4278 mm): Segment of C21 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(158.3500 mm, 87.1625 mm): Reference field of U5
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(157.7600 mm, 86.4278 mm): Segment of C25 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(157.7600 mm, 86.4278 mm): Segment of C25 on F.Silkscreen
    @(158.3500 mm, 87.1625 mm): Reference field of U5
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(158.7600 mm, 86.4278 mm): Segment of C24 on F.Silkscreen
    @(158.3500 mm, 87.1625 mm): Reference field of U5
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(176.1000 mm, 94.6500 mm): Reference field of U4
    @(175.6400 mm, 94.4922 mm): Segment of C9 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(170.1400 mm, 92.5900 mm): Segment of U4 on F.Silkscreen
    @(169.3100 mm, 93.0700 mm): Reference field of R11
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.5000 mm, 89.3800 mm): Reference field of R9
    @(171.5000 mm, 88.3300 mm): Reference field of R8
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.6536 mm, 88.5900 mm): Segment of R9 on F.Silkscreen
    @(171.5000 mm, 88.3300 mm): Reference field of R8
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.6536 mm, 87.8300 mm): Segment of R9 on F.Silkscreen
    @(171.5000 mm, 88.3300 mm): Reference field of R8
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.3464 mm, 89.8800 mm): Segment of R8 on F.Silkscreen
    @(171.5000 mm, 89.3800 mm): Reference field of R9
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(171.5000 mm, 89.3800 mm): Reference field of R9
    @(171.3464 mm, 89.1200 mm): Segment of R8 on F.Silkscreen
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(169.3100 mm, 93.0700 mm): Reference field of R11
    @(170.1400 mm, 92.9150 mm): Segment of U4 on F.Silkscreen
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(144.7300 mm, 100.3700 mm): Reference field of C16
    @(144.9532 mm, 99.8416 mm): Pad 1 [Net-(U2-VDDA)] of R18 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(144.7300 mm, 100.3700 mm): Reference field of C16
    @(144.9532 mm, 100.8616 mm): Pad 2 [Net-(U2-REGN)] of R18 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(129.2000 mm, 97.8000 mm): Reference field of TVS1
    @(130.4400 mm, 97.1900 mm): Pad 1 [Net-(J1-CC2)] of U1 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(145.8900 mm, 100.8500 mm): Pad 1 [-BATT] of C16 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.7632 mm, 100.7416 mm): Reference field of L1
    @(145.8900 mm, 99.8900 mm): Pad 2 [Net-(U2-VDDA)] of C16 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.7632 mm, 100.7416 mm): Reference field of L1
    @(145.8900 mm, 100.8500 mm): Pad 1 [-BATT] of C16 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(145.8900 mm, 99.8900 mm): Pad 2 [Net-(U2-VDDA)] of C16 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(145.8616 mm, 99.2693 mm): Polygon of U2 on F.Mask
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.1232 mm, 100.3516 mm): Reference field of R18
    @(145.5788 mm, 98.9865 mm): Polygon of U2 on F.Mask
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.7632 mm, 99.5345 mm): Segment of U2 on F.Silkscreen
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(142.5600 mm, 95.0800 mm): Reference field of C2
    @(143.0606 mm, 94.1394 mm): Pad 2 [-BATT] of C3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(127.2000 mm, 92.5800 mm): Reference field of C29
    @(128.1500 mm, 92.9000 mm): Pad 1 [-BATT] of C15 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(127.2000 mm, 92.5800 mm): Reference field of C29
    @(126.2500 mm, 92.9000 mm): Pad 2 [Net-(TVS1-A1)] of C15 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(187.6000 mm, 97.1000 mm): Reference field of C11
    @(189.0750 mm, 98.0000 mm): Pad 1 [-BATT] of C10 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(176.1000 mm, 94.6500 mm): Reference field of U4
    @(176.0000 mm, 94.1200 mm): Pad 1 [Net-(U4-BOOT)] of C9 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(177.1600 mm, 94.6000 mm): Reference field of C9
    @(177.8000 mm, 94.8000 mm): Pad 2 [Net-(D1-K)] of L2 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(187.6000 mm, 93.9000 mm): Reference field of C12
    @(186.1250 mm, 94.8000 mm): Pad 2 [Net-(C10-Pad2)] of C11 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(187.6000 mm, 93.9000 mm): Reference field of C12
    @(189.0750 mm, 94.8000 mm): Pad 1 [-BATT] of C11 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(187.6000 mm, 97.1000 mm): Reference field of C11
    @(186.1250 mm, 98.0000 mm): Pad 2 [Net-(C10-Pad2)] of C10 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(162.0938 mm, 108.0000 mm): Pad 3 [/SCL] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(162.0938 mm, 107.6000 mm): Pad 4 [/SDA] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(162.0938 mm, 107.2000 mm): Pad 5 [Net-(U3-CSN)] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(160.9000 mm, 108.0000 mm): Reference field of U3
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(160.9000 mm, 108.0000 mm): Pad 11 [-BATT] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(160.9000 mm, 108.0000 mm): Reference field of U3
    @(159.7062 mm, 108.4000 mm): Pad 9 [unconnected-(U3-THRM-Pad9)] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(160.9000 mm, 108.0000 mm): Reference field of U3
    @(159.7062 mm, 108.0000 mm): Pad 8 [/Fuel Gauge Alert] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(160.9000 mm, 108.0000 mm): Reference field of U3
    @(159.7062 mm, 107.6000 mm): Pad 7 [Net-(U3-REG)] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(169.6300 mm, 99.7000 mm): Reference field of R5
    @(168.7900 mm, 99.2000 mm): Pad 1 [-BATT] of R6 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(169.6300 mm, 99.7000 mm): Reference field of R5
    @(169.8100 mm, 99.2000 mm): Pad 2 [Net-(U4-FB)] of R6 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(173.0700 mm, 99.3000 mm): Reference field of R7
    @(173.0000 mm, 99.7600 mm): Pad 2 [-BATT] of C14 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(172.5200 mm, 99.7400 mm): Reference field of C13
    @(173.0000 mm, 99.7600 mm): Pad 2 [-BATT] of C14 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(173.0700 mm, 99.3000 mm): Reference field of R7
    @(173.0000 mm, 98.8000 mm): Pad 1 [Net-(U4-COMP)] of C14 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(172.5200 mm, 99.7400 mm): Reference field of C13
    @(171.9000 mm, 99.8100 mm): Pad 2 [Net-(C13-Pad1)] of R7 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(151.0400 mm, 105.4000 mm): Reference field of C6
    @(149.9632 mm, 105.1916 mm): Pad 2 [Net-(U2-SW2)] of L1 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(154.2000 mm, 110.7800 mm): Reference field of C28
    @(153.2500 mm, 111.1000 mm): Pad 2 [-BATT] of C30 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(156.9000 mm, 92.0000 mm): Reference field of C7
    @(156.4332 mm, 93.0166 mm): Polygon of Q1 on F.Mask
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(156.9000 mm, 92.0000 mm): Reference field of C7
    @(156.3682 mm, 92.8666 mm): PTH pad 12 [Net-(U2-SW2)] of Q1
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(159.9380 mm, 93.2250 mm): Reference field of Q5
    @(159.2000 mm, 93.4750 mm): Pad 1 [Net-(U2-VSYS)] of C7 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(156.4000 mm, 86.8000 mm): Pad 1 [+3.3V] of C21 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(156.2400 mm, 86.3200 mm): Reference field of C25
    @(156.4000 mm, 86.8000 mm): Pad 1 [+3.3V] of C21 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(159.7062 mm, 107.6000 mm): Pad 7 [Net-(U3-REG)] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(159.7062 mm, 107.2000 mm): Pad 6 [Net-(U3-CSP)] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(161.0000 mm, 107.4300 mm): Reference field of R17
    @(159.7062 mm, 108.0000 mm): Pad 8 [/Fuel Gauge Alert] of U3 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(155.5000 mm, 111.4600 mm): Reference field of J3
    @(155.1500 mm, 111.1000 mm): Pad 1 [+BATT] of C30 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(154.2000 mm, 110.7800 mm): Reference field of C28
    @(155.1500 mm, 111.1000 mm): Pad 1 [+BATT] of C30 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(156.2400 mm, 86.3200 mm): Reference field of C25
    @(156.4000 mm, 85.8400 mm): Pad 2 [-BATT] of C21 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(156.4000 mm, 85.8400 mm): Pad 2 [-BATT] of C21 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(157.4000 mm, 85.8400 mm): Pad 2 [-BATT] of C25 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(157.2400 mm, 86.3200 mm): Reference field of C24
    @(157.4000 mm, 86.8000 mm): Pad 1 [+3.3V] of C25 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(158.3500 mm, 87.1625 mm): Reference field of U5
    @(158.4000 mm, 86.8000 mm): Pad 1 [+3.3V] of C24 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(176.1000 mm, 94.6500 mm): Reference field of U4
    @(176.0000 mm, 95.0800 mm): Pad 2 [Net-(D1-K)] of C9 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(174.1600 mm, 99.2800 mm): Reference field of C14
    @(174.6050 mm, 97.2125 mm): Pad 8 [Net-(D1-K)] of U4 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(171.5000 mm, 88.3300 mm): Reference field of R8
    @(170.9900 mm, 88.2100 mm): Pad 2 [Net-(U4-EN)] of R9 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(171.5000 mm, 89.3800 mm): Reference field of R9
    @(170.9900 mm, 89.5000 mm): Pad 1 [Net-(U4-EN)] of R8 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(171.5000 mm, 89.3800 mm): Reference field of R9
    @(172.0100 mm, 89.5000 mm): Pad 2 [Net-(U2-VSYS)] of R8 on F.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(171.5000 mm, 88.3300 mm): Reference field of R8
    @(172.0100 mm, 88.2100 mm): Pad 1 [-BATT] of R9 on F.Cu
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(195.9536 mm, 95.0200 mm): Segment of R14 on B.Silkscreen
    @(195.8000 mm, 95.4300 mm): Reference field of R15
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(195.9536 mm, 95.7800 mm): Segment of R14 on B.Silkscreen
    @(195.8000 mm, 95.4300 mm): Reference field of R15
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.0000 mm, 102.4400 mm): Reference field of C27
    @(146.0000 mm, 101.4400 mm): Reference field of C26
[silk_overlap]: Silkscreen clearance
    Rule: board setup constraints silk; warning
    @(146.1078 mm, 102.9600 mm): Segment of C26 on B.Silkscreen
    @(146.0000 mm, 102.4400 mm): Reference field of C27
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(195.8000 mm, 95.4300 mm): Reference field of R15
    @(196.3100 mm, 95.4000 mm): Pad 1 [-BATT] of R14 on B.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(195.8000 mm, 95.4300 mm): Reference field of R15
    @(195.2900 mm, 95.4000 mm): Pad 2 [Net-(J2-CC2)] of R14 on B.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.0000 mm, 102.4400 mm): Reference field of C27
    @(145.5200 mm, 102.6000 mm): Pad 2 [-BATT] of C26 on B.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(146.0000 mm, 102.4400 mm): Reference field of C27
    @(146.4800 mm, 102.6000 mm): Pad 1 [Net-(U2-IADPT)] of C26 on B.Cu
[silk_over_copper]: Silkscreen clipped by solder mask
    Local override; warning
    @(145.5000 mm, 98.0300 mm): Reference field of R4
    @(145.4197 mm, 98.2263 mm): Via [-BATT] on F.Cu - B.Cu
[text_height]: Text height out of range (board setup constraints silk text height min height 0.8000 mm; actual 0.6400 mm)
    Rule: board setup constraints silk text height; warning
    @(137.9762 mm, 94.2980 mm): Reference field of Q4
[text_height]: Text height out of range (board setup constraints silk text height min height 0.8000 mm; actual 0.6400 mm)
    Rule: board setup constraints silk text height; warning
    @(138.0292 mm, 103.5980 mm): Reference field of Q3
[text_height]: Text height out of range (board setup constraints silk text height min height 0.8000 mm; actual 0.6400 mm)
    Rule: board setup constraints silk text height; warning
    @(155.5002 mm, 98.7352 mm): Reference field of Q2
[text_height]: Text height out of range (board setup constraints silk text height min height 0.8000 mm; actual 0.6400 mm)
    Rule: board setup constraints silk text height; warning
    @(155.5002 mm, 89.4852 mm): Reference field of Q1
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2373 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2381 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2381 mm)
    Rule: board setup constraints; warning
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2373 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2373 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(159.5480 mm, 95.4250 mm): PTH pad 9_3 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2381 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 95.8000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(160.4530 mm, 95.4250 mm): PTH pad 9_4 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2373 mm)
    Rule: board setup constraints; warning
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
    @(159.5480 mm, 97.3750 mm): PTH pad 9_6 [<no net>] of Q5
[hole_to_hole]: Drilled hole too close to other hole (board setup constraints min 0.2495 mm; actual 0.2381 mm)
    Rule: board setup constraints; warning
    @(160.4530 mm, 97.3750 mm): PTH pad 9_7 [<no net>] of Q5
    @(160.0000 mm, 97.0000 mm): Via [Net-(U2-SRP)] on F.Cu - B.Cu
[track_dangling]: Track has unconnected end
    Local override; warning
    @(178.0050 mm, 117.8750 mm): Track [/SDA] on F.Cu, length 0.0283 mm
[track_dangling]: Track has unconnected end
    Local override; warning
    @(154.8732 mm, 98.8916 mm): Track [Net-(U2-SRP)] on B.Cu, length 0.3900 mm

** Found 1 unconnected pads **
[unconnected_items]: Missing connection between items
    Local override; error
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0
    @(118.2500 mm, 89.7500 mm): Zone 'GND' [-BATT] on F.Cu and B.Cu, priority 0

** Found 22 Footprint errors **
[net_conflict]: No pad found for pin A1 (-BATT) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin B1 (-BATT) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin A6 (Net-(J1-D+-PadA6)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin B6 (Net-(J1-D+-PadA6)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin A7 (Net-(J1-D--PadA7)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin B7 (Net-(J1-D--PadA7)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin A8 (Net-(J1-SBU1)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin B8 (Net-(J1-SBU1)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin A4 (Net-(TVS1-A1)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin B4 (Net-(TVS1-A1)) in schematic
    Local override; warning
    @(121.0000 mm, 96.0000 mm): Footprint J1
[net_conflict]: No pad found for pin A1 (-BATT) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin B1 (-BATT) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin A4 (Net-(C10-Pad2)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin B4 (Net-(C10-Pad2)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin A6 (Net-(J2-D+-PadA6)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin B6 (Net-(J2-D+-PadA6)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin A7 (Net-(J2-D--PadA7)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin B7 (Net-(J2-D--PadA7)) in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin A8 in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin B8 in schematic
    Local override; warning
    @(196.7500 mm, 96.0000 mm): Footprint J2
[net_conflict]: No pad found for pin 33 (-BATT) in schematic
    Local override; warning
    @(146.7632 mm, 96.6000 mm): Footprint U2
[extra_footprint]: Extra footprint
    Local override; warning
    @(183.6000 mm, 102.0000 mm): Footprint OUT

** Ignored checks **
    - Footprint has no courtyard defined
    - Track endpoint not centered on via
    - Tuning profile track geometries
    - Footprint doesn't match symbol's footprint filters
    - Footprint component type doesn't match footprint pads

** End of Report **
